**Section 201.600 Applicability**

An owner or operator of a source seeking a PBR for a new or modified boiler is eligible to obtain a PBR under this Subpart N if:

a) The boiler has a maximum design heat input capacity of:

1) Less than or equal to 50 MMBtu/hr; or

2) Greater than 50 MMBtu/hr and less than or equal to 100 MMBtu/hr and is equipped with low-NOx burners designed by the manufacturer to meet a NOx emission limit of not greater than 0.05 lb/MMBtu;

b) The boiler primarily burns pipeline natural gas, butane, propane, or refinery fuel gas;

c) The only backup or reserve fuel burned in the boiler is diesel fuel, butane, or propane. If diesel fuel is the backup fuel, the burning of diesel fuel in the boiler must be such that, as appropriate, the boiler is a "unit designed to burn gas 1 subcategory," as defined by 40 CFR 63.7575, or a "gas-fired boiler," as defined by 40 CFR 63.11237 as incorporated by reference in Section 201.104; and

d) The emissions from the boiler consist entirely of the products of fuel combustion.

(Source: Added at 41 Ill. Reg. 4140, effective March 24, 2017)