**Section 207.312 Operability Check**

Each vehicle that is to be retired pursuant to this Part shall pass an operability check prior to purchase and collection. The operability check shall include, at a minimum:

a) Start-up of the vehicle;

b) Test-drive of the vehicle for five or more feet in forward gear;

c) Test-drive of the vehicle for five or more feet in reverse gear;

d) Shut-off of the vehicle; and

e) Visual inspection for fluid leakage or any malfunction or other damage that would render the vehicle unsuitable for normal operation.