**Section 211.670 Baked Coatings**

"Baked coatings" means any coating which is cured or dried in an oven where the oven air temperature exceeds 90ºC (194ºF), or any coating which is cured in any manner that does not otherwise fit into the definition of "air dried coatings," as defined in Section 211.330 of this Part.

(Source: Amended at 19 Ill. Reg. 6823, effective May 9, 1995)