**Section 211.2810 Heated Airless Spray**

"Heated airless spray" means an airless spray coating method in which the coating is heated just prior to application.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)