**Section 211.2825 Heat-Resistant Coating**

"Heat-resistant coating" means, for purposes of 35 Ill. Adm. Code 218 and 219, a coating that must withstand a temperature of at least 204oC (400oF) during normal use.

(Source: Added at 34 Ill. Reg. 14119, effective September 14, 2010)