**Section 211.2955 High Bake Coating**

"High bake coating" means, for purposes of 35 Ill. Adm. Code 218 and 219, a coating that is designed to cure only at temperatures of more than 90oC (194oF).

(Source: Added at 34 Ill. Reg. 14119, effective September 14, 2010)