**Section 211.5330 Purged Process Fluid**

"Purged process fluid" means liquid or vapor from a process unit that contains volatile organic material and that results from flushing or cleaning the sample line(s) of a process unit so that an uncontaminated sample may then be taken for testing or analysis

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)