**Section 212.205 Coal-fired Industrial Boilers For Which Construction or Modification Commenced Prior to April 14, 1972, Equipped with Flue Gas Desulfurization Systems**

Notwithstanding Sections 212.201 through 212.204 of this Subpart, no person shall cause or allow the emission of particulate matter into the atmosphere from coal-fired industrial boilers equipped with flue gas desulfurization systems for which construction or modification commenced prior to April 14, 1972, to exceed 0.39 kg of particulate matter per MW-hr of actual heat input in any one-hour period (0.25 lbs/mmbtu). Nothing in this rule shall be construed to prevent compliance with applicable regulations promulgated by the USEPA under Section 111 of the CAA as amended. *The provisions of Section 111 of the Clean Air Act relating to standards of performance for new stationary sources...are applicable in this State and are enforceable under* *the Act* [415 ILCS 5/9.1(b)].

(Source: Amended at 20 Ill. Reg. 7605, effective May 22, 1996)