**Section 214.561 E. D. Edwards Electric Generating Station**

Sulfur dioxide emissions from Boiler Nos. 1, 2, and 3 at the Edwards Station may not exceed the limits listed in this Section. CILCO must determine compliance with these limits on a daily basis using the sulfur dioxide methodology of the Phase II Acid Rain Program set forth in 40 CFR 75.

a) The average sulfur dioxide emissions from Boiler Nos. 1, 2, and 3, as a group may not exceed 4.71 pounds per million British thermal units (lb/mmBtu) of actual heat input;

b) The average sulfur dioxide emissions from any one boiler may not exceed 6.6 lb/mmBtu of actual heat input; and

c) Sulfur dioxide emissions for all three boilers, as a group, may not exceed 34,613 pounds per hour, on a 24-hour average basis.

(Source: Amended at 27 Ill. Reg. 12101, effective July 11, 2003)