**Section 218.142 Pumps and Compressors**

No person shall cause or allow the discharge of more than 32.8 ml (2 cu in) of VOL with vapor pressure of 17.24 kPa (2.5 psia) or greater at 294.3° K (70° F) into the atmosphere from any pump or compressor in any 15 minute period at standard conditions.