**Section 218.980 Applicability**

a) Maximum theoretical emissions:

1) A source is subject to this Subpart if it contains process emission units not regulated by Subparts B, E, F (excluding Section 218.204(l) of this Part), H (excluding Section 218.405 of this Part), Q, R, S, T (excluding Section 218.486 of this Part), V, X, Y, Z or BB of this Part, which as a group both:

A) Have maximum theoretical emissions of 90.7 Mg (100 tons) or more per calendar year of VOM, and

B) Are not limited to less than 90.7 Mg (100 tons) of VOM emissions per calendar year in the absence of air pollution control equipment through production or capacity limitations contained in a federally enforceable permit or a SIP revision.

2) If a source is subject to this Subpart as provided in this Subpart, the requirements of this Subpart shall apply to a source's VOM emission units which are not included within any of the categories specified in Subparts B, E, F, H, Q, R, S, T, V, X, Y, Z, AA, BB, PP, QQ, or RR of this Part or which are not exempted from permitting requirements pursuant to 35 Ill. Adm. Code 201.146.

b) Potential to emit:

1) A source is subject to this Subpart if it has the potential to emit 22.7 Mg (25 tons) or more of VOM per year, in aggregate, from emission units, other than furnaces at glass container manufacturing sources and VOM leaks from components, that are:

A) Not regulated by Subparts B, E, F, H, Q, R, S, T, (excluding Section 218.486 of this Part), V, X, Y, Z, or BB of this Part, or

B) Not included in any of the following categories: synthetic organic chemical manufacturing industry (SOCMI) distillation, SOCMI reactors, wood furniture, plastic parts coating (business machines), plastic parts coating (other), offset lithography, industrial wastewater, autobody refinishing, SOCMI batch processing, volatile organic liquid storage tanks and clean-up solvents operations.

2) If a source is subject to this Subpart as provided above, the requirements of this Subpart shall apply to a source's VOM emission units, which are:

A) Not included within any of the categories specified in Subparts B, E, F, H, Q, R, S, T, V, X, Y, Z, AA, BB, CC, DD, PP, QQ or RR of this Part, or which are not exempted from permitting requirements pursuant to 35 Ill. Adm. Code 201.146 (excluding Section 201.146(o) and (p)), or

B) Not included in any of the following categories: synthetic organic chemical manufacturing industry (SOCMI) distillation, SOCMI reactors, wood furniture, plastic parts coating (business machines), plastic parts coating (other), offset lithography, industrial wastewater, autobody refinishing, SOCMI batch processing, volatile organic liquid storage tanks and clean-up solvents operations.

c) If a source ceases to fulfill the criteria of subsections (a) and/or (b) of this Section, the requirements of this Subpart shall continue to apply to an emission unit which was ever subject to the control requirements of Section 218.986 of this Part.

d) No limits under this Subpart shall apply to emission units with emissions of VOM to the atmosphere less than or equal to 2.3 Mg (2.5 tons) per calendar year if the total emissions from such emission units not complying with Section 218.986 of this Part does not exceed 4.5 Mg (5.0 tons) per calendar year.

e) For the purposes of this Subpart, an emission unit shall be considered regulated by a Subpart, if it is subject to the limits of that Subpart. An emission unit is considered not regulated by a Subpart if it is not subject to the limits of that Subpart, e.g., the emission unit is covered by an exemption in the Subpart or the applicability criteria of the Subpart are not met.

f) The control requirements in Subpart TT shall not apply to sewage treatment plants; vegetable oil extraction and processing; coke ovens (including by-product recovery plants); fuel combustion units; bakeries; barge loading facilities; jet engine test cells; production of polystyrene foam insulation board including storage and extrusion of scrap where blowing agent is added to the polystyrene resin at the source, but not including blending and preliminary expansion of resin prior to molding where blowing agent is incorporated into the polystyrene resin by the producer of the resin; production of polystyrene or polyethylene foam packaging not including blending and preliminary expansion of resin prior to molding where blowing agent is incorporated into the polystyrene or polyethylene resin by the producer of the resin, and not including storage and extrusion of scrap where blowing agent is added to the polystyrene or polyethylene resin at the source; and iron and steel production; and furnaces at glass container manufacturing sources.

(Source: Amended at 20 Ill. Reg. 14428, effective October 17, 1996)