**Section 229.156 Violations by HMIWIs Equipped with a Wet Scrubber**

Except as provided in Section 229.164 of this Subpart, for an HMIWI equipped with a wet scrubber:

a) Simultaneous operation of an HMIWI above the maximum charge rate and below the minimum pressure drop across the wet scrubber or below the minimum horsepower or amperage to the system (each measured on a 3-hour rolling average) is a violation of the PM emissions limit;

b) Simultaneous operation of an HMIWI above the maximum charge rate and below the minimum secondary chamber temperature (each measured on a 3-hour rolling average) is a violation of the CO emissions limit;

c) Simultaneous operation of an HMIWI above the maximum charge rate, below the minimum secondary chamber temperature and below the minimum scrubber liquor flow rate (each measured on a 3-hour rolling average) is a violation of the dioxin/furan emissions limit;

d) Simultaneous operation of an HMIWI above the maximum charge rate and below the minimum scrubber liquor pH (each measured on a 3-hour rolling average) is a violation of the HCl emissions limit;

e) Simultaneous operation of an HMIWI above the maximum flue gas temperature and above the maximum charge rate (each measured on a 3-hour rolling average) is a violation of the Hg emissions limit;

f) Use of the bypass stack at any time during operation of an HMIWI is a violation of the PM, dioxin/furan, HCl, Pb, Cd and Hg emissions limits;

g) If a CO CEMS is used to determine compliance with a CO emissions limit, operation of the HMIWI above the CO emissions limit as measured by the CO CEMS shall be a violation of the emissions limit;

h) If a CEMS is used to determine compliance with a PM, HCl, Pb, Cd, and/or Hg emissions limit, operation of the HMIWI above the applicable emissions limit as measured by the CEMS shall be a violation of the emissions limit;

i) If a continuous automated sampling system is used, operation of the HMIWI above the dioxin/furan emissions limit as measured by the continuous automated sampling system shall be a violation of the dioxin/furan emissions limit; or

j) If a continuous automated sampling system is used, operation of the HMIWI above the Hg emissions limit as measured by the continuous automated sampling system shall be a violation of the Hg emissions limit.

(Source: Amended at 35 Ill. Reg. 16615, effective September 30, 2011)