SUBPART J: REQUIREMENTS FOR HMIWI OPERATORS