SUBPART E: TRANSIENT LOADED MODE TEST EMISSION STANDARDS