SUBPART F: EVAPORATIVE TEST STANDARDS