**Section 240.182 On-Road Remote Sensing Emission Standards**

Exhaust emissions shall not exceed the following limitations:

|  |  |  |
| --- | --- | --- |
| Model Year | Hydrocarbons(ppm) | Carbon Monoxide(%) |
| 1996 and newer | 400 | 2.0 |

(Source: Amended at 35 Ill. Reg. 5552, effective March 18, 2011)