**Section 240.202 Visual Inspection Test Standards**

Vehicles subject to visual inspection testing shall fail the visual inspection test if the MIL does not illuminate in the key-on/engine off position or continuously illuminates in the key-on/engine on position.

(Source: Added at 36 Ill. Reg. 1066, effective February 1, 2012)