**Section 266.110 Allowable Emission Rate for Small Operations**

For process weight rates of less than 100 pounds per hour (45.35 kg/hr), the allowable emissions rate is 0.55 pounds per hour (0.25 kg/hr).