PART 306

PERFORMANCE CRITERIA