**Section 307.2704 Glycerine Concentration**

a) Applicability. This Section applies to discharges resulting from the concentration of sweet water from saponification or fat splitting to approximately 60 to 80 percent crude glycerine content.

b) Specialized Definitions. The Board incorporates by reference 40 CFR 417.41 (2003). This incorporation includes no later amendments or editions.

c) Existing Sources

1) The Board incorporates by reference 40 CFR 417.44 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (c)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

d) New Sources

1) The Board incorporates by reference 40 CFR 417.46 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (d)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

3) "New source" means any building, structure, facility, or installation whose construction commenced after December 26, 1973.

(Source: Amended at 47 Ill. Reg. 4662, effective March 23, 2023)