PART 375

COMBINED SEWER OVERFLOW EXCEPTION CRITERIA

AND FIRST FLUSH DETERMINATION