**Section 611.974 Additional Requirements for Consecutive Systems**

If a supplier has a consecutive system that does not add a disinfectant but which delivers water that has been treated with a primary or residual disinfectant other than ultraviolet light, it must comply with the analytical and monitoring requirements for chlorine and chloramines in Sections 611.381(c) and 611.382(c)(1) and with the compliance requirements in Section 611.383(c)(1), and the supplier must report monitoring results pursuant to Section 611.384(c).

BOARD NOTE: Derived from 40 CFR 141.624 (2012).

(Source: Amended at 37 Ill. Reg. 1978, effective February 4, 2013)