**Section 652.220 Corrosion Prevention at Community Water Supplies**

a) A community water supply must use *protective coatings personnel to carry out corrosion prevention and mitigation methods* on the following:

1) *exposed water treatment tanks, exposed non-concrete water treatment structures, exposed water treatment pipe galleys;*

2) *exposed pumps; and*

3) *generators*. [415 ILCS 5/14.7(a)(2)(A)]

b) A community water supply must use *inspectors to ensure that best practices and standards* specified in Section 652.210 *are adhered to on each corrosion prevention project* under this Part [415 ILCS 5/14.7(a)(2)(B)].