**Section 653.106 Distribution System Pressure**

a) Distribution system design shall conform to the Standards.

b) Distribution systems shall be designed to maintain a minimum pressure of 20 psi measured at the ground surface in all parts of the system under fire-fighting demand or other similar emergency operating conditions.