**Section 653.120 Piping Identification**

a) Piping in a water treatment facility shall be identified clearly by legends and color coding as described in the Standards or American National Standards Institute (ANSI) Standard A-13.1. A consistant standard shall be used throughout the system.

b) Potable water lines shall be clearly and permanently identified where dual water lines or pressure sewer systems exist.