SUBPART B: PROCEDURES FOR DETERMINING THE LATERAL AREA OF INFLUENCE OF WELLS UNDER NORMAL OPERATIONAL CONDITIONS