**Section 704.185 Operation Requirements**

The permit must establish any maximum injection volumes and pressures necessary to assure that fractures are not initiated in the confining zone, that injected fluids do not migrate into any USDW, that formation fluids are not displaced into any USDW, and to assure compliance with the 35 Ill. Adm. Code 730 operating requirements.

BOARD NOTE: Derived from 40 CFR 144.52(a)(3) (2005).

(Source: Amended at 31 Ill. Reg. 605, effective December 20, 2006)