**Section 721.982 Standards: General**

a) This Section applies to the management of hazardous secondary material in tanks and containers subject to this Subpart CC.

b) The remanufacturer or other person that stores or treats the hazardous secondary material must control air pollutant emissions from each hazardous secondary material management unit in accordance with standards specified in Sections 721.984 through 721.987, as applicable to the hazardous secondary material management unit, except as provided for in subsection (c).

c) A tank or container is exempt from standards specified in Sections 721.984 through 721.987, as applicable, provided that the hazardous secondary material management unit is a tank or container for which all hazardous secondary material entering the unit has an average VO concentration at the point of material origination of less than 500 parts per million by weight (ppmw). The average VO concentration must be determined using the procedures specified in Section 721.983(a). The remanufacturer or other person that stores or treats the hazardous secondary material must review and update, as necessary, this determination at least once every 12 months following the date of the initial determination for the hazardous secondary material streams entering the unit.

(Source: Added at 40 Ill. Reg. 11367, effective August 9, 2016)