**Section 724.298 Special Requirements for Ignitable or Reactive Waste**

a) Ignitable or reactive waste must not be placed in tank systems unless the following is true:

1) The waste is treated, rendered, or mixed before or immediately after placement in the tank system so that the following is true:

A) The resulting waste, mixture, or dissolved material no longer meets the definition of ignitable or reactive waste under 35 Ill. Adm. Code 721.121 or 721.123; and

B) Section 724.117(b) is complied with; or

2) The waste is stored or treated in such a way that it is protected from any material or conditions that may cause the waste to ignite or react; or

3) The tank is used solely for emergencies.

b) The owner or operator of a facility where ignitable or reactive waste is stored or treated in a tank must comply with the requirements for the maintenance of protective distances between the waste management area and any public ways, streets, alleys, or an adjoining property line that can be built upon, as required in tables 2-1 through 2-6 of "Flammable and Combustible Liquids Code", NFPA 30, incorporated by reference in 35 Ill. Adm. Code 720.111(a).

(Source: Amended at 42 Ill. Reg. 22614, effective November 19, 2018)