**Section 725.954 Standards: Pressure Relief Devices in Gas/Vapor Service**

a) Except during pressure releases, each pressure relief device in gas/vapor service must be operated with no detectable emissions, as indicated by an instrument reading of less than 500 ppm above background as measured by the method specified in Section 725.963(c).

b) Actions Following Pressure Release

1) After each pressure release, the pressure relief device must be returned to a condition of no detectable emissions, as indicated by an instrument reading of less than 500 ppm above background, as soon as practicable, but no later than 5 calendar days after each pressure release, except as provided in Section 725.959.

2) No later than five calendar days after the pressure release, the pressure relief device must be monitored to confirm the condition of no detectable emissions, as indicated by an instrument reading of less than 500 ppm above background, as measured by the method specified in Section 725.963(c).

c) Any pressure relief device that is equipped with a closed-vent system capable of capturing and transporting leakage from the pressure relief device to a control device as described in Section 725.960 is exempt from the requirements of subsections (a) and (b).

(Source: Amended at 42 Ill. Reg. 23725, effective November 19, 2018)