SUBPART C: CRITERIA AND STANDARDS APPLICABLE

TO CLASS II INJECTION WELLS