**Section 734.APPENDIX C Backfill Volumes**

|  |  |  |
| --- | --- | --- |
| Volume of Tank in Gallons | Maximum amount of backfill material to be removed:Cubic yards | Maximum amount of backfill material to be replaced:Cubic yards |
| <285285 to 299300 to 559560 to 9991000 to 10491050 to 11491150 to 19992000 to 24992500 to 29993000 to 39994000 to 49995000 to 59996000 to 74997500 to 82998300 to 999910,000 to 11,99912,000 to 14,999>15,000 | 54555667818994112128143175189198206219252286345 | 565758708796101124143161198219235250268312357420 |

A conversion factor of 1.5 tons per cubic yard must be used to convert tons to cubic yards.