**Section 902.120 Standards Applicable to all Passenger Cars and to Other Motor Vehicles with Gross Vehicle Weight (GVW) of 8,000 Pounds or Less**

a) This Section applies to all passenger cars regardless of weight and to other motor vehicles with a GVW of 8,000 pounds or less, except motorcycles and motor driven cycles.

b) Operation of a motor vehicle subject to this Section at any time under any conditions of highway grade, load, acceleration or deceleration must not exceed the following limits:

1) On highways with speed limits of 35 miles per hour or less, 74 dB(A), or 76 dB(A) when operating on a grade exceeding 3%, measured with fast meter response at 50 feet from the centerline of lane of travel;

2) On highways with speed limits of more than 35 miles per hour, 82 dB(A), or 85 dB(A) if the vehicle is equipped with two or more snow or mud/snow tires, measured with fast meter response at 50 feet from the centerline of lane of travel.

(Source: Amended at 42 Ill. Reg. 20474, effective November 1, 2018)