**Section 902.121 Standards Applicable to Motor Vehicles with GVW in Excess of 8,000 Pounds**

a) This Section applies to motor vehicles with a GVW in excess of 8,000 pounds.

b) Operation of a motor vehicle subject to this Section at any time under any conditions of highway grade, load, acceleration or deceleration must not exceed the limits at 40 CFR 202.20(a), incorporated by reference at 35 Ill. Adm. Code 900.106.

c) Operation of a motor vehicle subject to this Section, powered by an engine with an engine speed governor, must not exceed the standard for operation under the stationary test at 40 CFR 202.21(a), incorporated by reference at 35 Ill. Adm. Code 900.106.

(Source: Amended at 42 Ill. Reg. 20474, effective November 1, 2018)