**Section 370.2820 Emergency Electrical System**

An emergency electrical service, which may be battery operated if effective for four (4) or more hours, shall provide services as follows:

a) Illumination of means of egress

b) Fire detection and alarm system

c) Telephone service

d) Exit sign fixtures