**Section 518.TABLE A Piping Locations for Oxygen, Vacuum and Medical Compressed Air**

|  |  |  |  |
| --- | --- | --- | --- |
| Location | Oxygen | Vacuum | Compressed Air |
|   |  |  |  |
| Patient Treatment Room | A | A |  |
| Examination and Treatment Rooms | D | D |  |
|  |  |  |  |

A = One outlet accessible to each bed. One outlet may serve 2 beds.

D = One outlet.

(Source: Amended at 33 Ill. Reg. 8317, effective June 4, 2009)