**Section 785.515 Preheaters**

The preheaters shall be of stainless steel or other equally corrosion-resistant material, cleanable, accessible for inspection and shall be equipped with automatic temperature controls.