**Section 785.765 Press**

The cheese press shall be constructed of stainless steel and all joints welded and all surfaces, seams, and openings readily cleanable. The pressure advice shall be the continuous type. Press cloths shall be maintained in good repair and in a sanitary condition. Single-service press cloths shall be used only once.

(Source: Adopted at 11 Ill. Reg. 2356, effective February 1, 1987)