**Section 845.270 Prohibited Work Practices**

No person conducting lead abatement or lead mitigation shall employ any of the following methods:

a) Open flame burning;

b) Dry sanding;

c) Open abrasive blasting;

d) Uncontained exterior hydro-blasting;

e) Interior hydro-blasting;

f) Methylene chloride application; or

g) Dry scraping.

(Source: Amended at 43 Ill. Reg. 2440, effective February 8, 2019)