SUBPART A: DEFINITIONS AND INCORPORATED MATERIALS

Section

860.10 Definitions

860.20 Incorporated and Referenced Materials

SUBPART B: PERMITS

Section

860.100 Required Permits

860.110 Applications

860.120 Plans

860.130 Flood Plain Requirements

860.140 Occupancy of New Sites

860.150 Immobilization

860.160 Deletion of Sites

SUBPART C: REQUIREMENTS OF THE MANUFACTURED HOME COMMUNITY

Section

860.200 Layout of the Manufactured Home Community

860.210 Support Systems

860.220 Streets and Parking

860.230 Water

860.240 Sewage

860.250 Electrical

860.260 Fuel Supply

860.270 Fire Safety

860.280 Lighting

860.290 Pools and Beaches

860.300 Solid and Landscape Waste

860.310 Manufactured Home Community Appearance

860.320 Identification of Sites

860.330 Vector Control

860.340 Fences

860.350 Inspection Doors

860.360 Recreational Vehicles

860.370 Animal Control

860.380 Vacant Sites

860.390 Duplex Units

SUBPART D: ADDITIONAL RESPONSIBILITIES OF THE LICENSEE

Section

860.400 Required Documents

860.410 Manufactured Home Community Rules

860.420 Register

860.430 Inspections by Manufactured Home Community Management

SUBPART E: ADMINISTRATIVE ACTION BY THE DEPARTMENT

Section

860.500 Variance Procedures

860.510 Enforcement Action

860.520 Common Operation

860.530 Existing Communities

860.540 Administrative Monetary Penalties

860.ILLUSTRATION A Manufactured Home Community Layout For Sites Constructed After July 1, 1998

860.ILLUSTRATION B Typical Manufactured Home Site

860.ILLUSTRATION C Water Service Connection

860.ILLUSTRATION D Sewer Service Connection

860.ILLUSTRATION E Sample Register Information

860.ILLUSTRATION F Manufactured Home Community Electrical System

860.APPENDIX A Regional Offices of the Department

860.APPENDIX B Explanation of the 1996 National Electrical Code Requirements for Manufactured Home Communities (Repealed)

860.APPENDIX C Unlicensed Motor Vehicles

860.APPENDIX D Home Rule Units (Repealed)

860.TABLE A Minimum Road Width

860.TABLE B Water Distribution Pipe Size

860.TABLE C Minimum Size and Slope of Sewer Mains