SUBPART A: DEFINITIONS AND INCORPORATED MATERIALS

Section

870.10 Definitions

870.20 Incorporated and Referenced Materials

SUBPART B: MANUFACTURED HOME INSTALLER ACCREDITATION COURSES

Section

870.30 Accreditation of Manufactured Home Installer Course

870.40 Responsibilities of Entities Offering Accredited Manufactured Home Installer Courses

870.50 Requirements for Accredited Manufactured Home Installer Course Curriculum

870.55 Reciprocity

870.60 Revocation of Accreditation

SUBPART C: MANUFACTURED HOME INSTALLER REQUIREMENTS

Section

870.65 Requirements for Manufactured Home Installers License

870.70 Continuing Education

870.80 Installation Seals and Compliance Certificates

SUBPART D: REQUIREMENTS FOR THE INSTALLATION

OF MANUFACTURED HOMES

Section

870.90 Requirements for the Installation of Manufactured Homes

870.100 Site Location

870.110 Support Systems

870.120 Structural Connections, Sealing and Patching

870.130 Electrical Hookup of Manufactured Homes

870.140 Plumbing

870.150 Heating and Air Conditioning

870.160 Natural and Liquefied Petroleum Gas Installation

870.170 Perimeter Enclosures

SUBPART E: MANUFACTURED HOME ANCHORING

Section

870.190 Tiedown Equipment Approval

870.200 Equipment Specifications

870.210 Compliance

870.220 Tiedown Installation Requirements

SUBPART F: MANUFACTURERS OF MANUFACTURED HOMES

Section

870.230 Manufacturer's Responsibilities

SUBPART G: ADMINISTRATIVE HEARINGS

Section

870.240 Penalties

870.250 Injunctive Relief

870.TABLE A Soil Pressure

870.TABLE B Footing Areas Required for Soil's Load-Bearing Capacity − Design Roof Load 20 Pounds Per Square Foot

870.TABLE C Footing Areas Required for Soil's Load-Bearing Capacity − Design n Roof Load 30 Pounds Per Square Foot

870.TABLE D Footing Areas Required for Soil's Load-Bearing Capacity − Design Roof Load 40 Pounds Per Square Foot

870.TABLE E Pier Load and Minimum Pier Capacity for 12 Foot Wide Section (Pounds)

870.TABLE F Pier Load and Minimum Pier Capacity for 14 Foot Wide Section (Pounds)

870.TABLE G Pier Load and Minimum Pier Capacity for 16 Foot Wide Section (Pounds)

870.TABLE H Multi-Section Fastening Schedule