**Section 870.TABLE H Multi-Section Fastening Schedule**

| **CONNECTOR LOCATION** | **FASTENER SIZE** | **FASTENER ANGLE** | **FASTENER SPACING** |
| --- | --- | --- | --- |
| Roof ridge beam connection | ½ inch carriage bolts | 90 degrees | 48 inches on center |
| Roof ridge beam connection | ⅜ inch lag screws with washers | 45 degrees or less | 24 inches on center |
| Roof rafter connection | 4 inch by 10 inch 18 gauge straps with 10-10d nails | 90 degrees | 48 inches on center |
| Floor rim joist connection | ⅜ inch lag screws with washers | 45 degrees or less | 32 inches on center |
| Floor connection | Marriage clips | 90 degrees | Where installed |