**Section 890.190 Piping Measurements**

Except where otherwise specified in this Part, all measurements between pipes, or between pipes and walls or footings, shall be made from the outside edge nearest the parallel pipe, wall or footing.

(Source: Amended at 38 Ill. Reg. 9940, effective April 24, 2014)