**Section 890.430 Cleanout Equivalent**

Fixture Trap. A fixture trap, readily removable and without disturbing concealed plumbing or requiring fixture removal, is acceptable as a cleanout equivalent, if there is no more than one (1) 90 degree bend on the line to be rodded. A water closet is not considered a cleanout equivalent.

(Source: Amended at 22 Ill. Reg. 21540, effective December 1, 1998)