**Section 890.750 Hydromassage/Whirlpool Bathtubs**

a) Whirlpool bathtubs shall be installed so that the tub, pump, jets and pump tubing drain completely after each use. The pump shall be located above the weir of the whirlpool tub trap.

b) All whirlpool bathtubs shall comply with ASME A112.19.7/CSA 45.10 (Whirlpool Bathtub Appliances). The suction fittings used in whirlpool bathtubs shall conform to ANSI/APSP 16 (Standard Suction Fittings for Use in Swimming Pools, Wading Pools, Spas, and Hot Tubs).

(Source: Amended at 38 Ill. Reg. 9940, effective April 24, 2014)