**Section 890.1710 General Requirements**

a) All material, fittings, appurtenances and devices shall be in accordance with standards listed in Appendix A, Table A.

b) The drainage and venting for security fixtures shall be in accordance with Sections 890.910 through 890.930, 890.1010 through 890.1060, 890.1310 through 890.1380 and Sections 890.1410 through 890.1600.

c) The water supply for security fixtures shall be in accordance with Sections 890.1110 through 890.1240. Note: A full-way valve for each cell shall be located outside the cell.