Section

900.10 Definitions

900.15 Incorporated and Referenced Materials

900.20 General Requirements

900.30 Special Requirements

900.35 Revised Total Coliform Rule for Non-Community Public Water Systems

900.40 Water System Design

900.45 Non-Transient, Non-Community Public Water System Operator Certification

900.50 Inorganic Chemicals (Repealed)

900.60 Turbidity (Repealed)

900.65 Organic Chemicals (Repealed)

900.70 Microbiological (Repealed)

900.80 Public Notification (Repealed)

900.90 Record Maintenance and Reporting (Repealed)

900.100 Variances and Exemptions (Repealed)

900.TABLE A Sources of Pollution in Location to Wells and/or Finished Water Storage Facilities

900.TABLE B Design Capacity for a Non/Community Public Water System

900.TABLE C Pressure Factors

900.TABLE D Coliform Sampling Frequency According to Population Served (Repealed)

900.TABLE E Lead and Copper Sampling Frequency-Requirements for First Year of Sampling (Repealed)

900.TABLE F Lead and Copper Sampling Frequency-Requirements After First Year of Sampling (Repealed)

900.TABLE G Water Quality Sampling Requirements (Repealed)

900.TABLE H Water Quality Sampling Requirements-Reduced Sampling (Repealed)

900.TABLE I Table of Factors to be Used in Saturation Index Calculations (Repealed)

900.EXHIBIT A Values of A Based Upon Total Solids (Repealed)

900.EXHIBIT B Values of B Based Upon Water Temperature (Repealed)

900.EXHIBIT C Values of C Based Upon Calcium Hardness Expressed as CaCO3 (Repealed)

900.EXHIBIT D Values of D Based Upon Alkalinity Expressed as CaCO3 (Repealed)