Section

906.10 Applicability

906.20 Definitions

906.25 Incorporated Materials

906.30 Soil and Site Requirements

906.40 Fill Material

906.50 Mound Design

906.60 Distribution System (for sewage flows of less than 800 gallons per day)

906.70 Distribution System (for sewage flows in excess of 800 gallons per day)

906.APPENDIX A Illustrations and Exhibits

906.ILLUSTRATION A Plan View of a Mound Utilizing Two Trenches as the Absorption Area

906.ILLUSTRATION B Cross-Section of a Mound Using Trenches for the Absorption Area

906.ILLUSTRATION C Plan View of a Mound Utilizing a Bed as the Absorption Area

906.ILLUSTRATION D Cross-Section of a Mound Using a Bed for the Absorption Area

906.ILLUSTRATION E Mound Distribution System

906.ILLUSTRATION F Typical Pumping Chamber

906.ILLUSTRATION G Tee-To-Tee Lateral/Manifold Construction

906.ILLUSTRATION H Dosing Frequencies for Various Soil Textures

906.ILLUSTRATION I Maximum Manifold Length (ft) for Various Manifold Diameters Given the Lateral Discharge Rate and Lateral Spacing

906.EXHIBIT A Soil and Site Factors that Restrict Mound Systems

906.EXHIBIT B Fine Aggregate Gradations

906.EXHIBIT C Downslope and Upslope Width Corrections for Mounds on Sloping Sites

906.EXHIBIT D Allowable Lateral Lengths (Feet) for Three Pipe Diameters, Three Perforation Sizes, and Two Perforation Spacings (Use design method in Section 906.60 if system is to treat flow from more than 4 bedrooms)

906.EXHIBIT E Dosing Quantity for Various Sized Homes

906.EXHIBIT F Void Volume for Various Diameter Pipes

906.EXHIBIT G Pumping Chamber Sizes for Various Sized Homes

906.EXHIBIT H Perforation Discharge Rates in Gallons per Minute Versus Perforation Diameter and In-Line Pressure

906.EXHIBIT I Friction Loss in Schedule 40 Plastic Pipe