Section

920.10 Definitions

920.15 Incorporated and Referenced Materials

920.20 Scope

920.30 General Requirements

920.40 Design Factors

920.50 Location

920.60 Drilled Wells in Unconsolidated Formations

920.70 Drilled Well Construction in Consolidated Formations

920.80 Special Type Wells

920.90 Construction Materials and Other Requirements

920.100 Finishing and Testing

920.110 Non-Compliant Existing Wells

920.120 Abandoned Wells

920.130 Water Well Permit Requirements

920.140 Administrative Hearings

920.150 Designation of Agents of the Department

920.160 Issuance of Water Well and Closed Loop Well Permits by Units of Local Government or Local Health Departments

920.170 Monitoring Wells

920.180 Closed Loop Wells

920.190 Assurance of Potable Water Supply

920.200 Closed Loop Well System Permit Requirements

920.210 Examination for Closed Loop Well Contractor Certification and Fees

920.220 Closed Loop Contractor Registration, Renewal and Fees

920.230 Registered Closed Loop Well Contractor Responsibility

920.240 Closed Loop Well Continuing Education Sessions

920.250 Approval of Closed Loop Well Third Party Organizations

920.ILLUSTRATION A Unconsolidated Formations: Oversized Drill Hole

920.ILLUSTRATION B Unconsolidated Formations: Mechanically Driven Casing

920.ILLUSTRATION C Gravel Pack Construction

920.ILLUSTRATION D Creviced Formations: Earth Cover Less Than 30 Feet Thick

920.ILLUSTRATION E Creviced Formations: Earth Mantle Cover Over 30 Feet Thick − Oversized Drill Hole

920.ILLUSTRATION F Creviced Formations: Earth Cover Over 30 Feet Thick − Mechanically Driven Casing

920.ILLUSTRATION G Bored or Dug Well − Well Not Finished With Buried Slab

920.ILLUSTRATION H Bored or Dug Well − Buried Slab Construction

920.ILLUSTRATION I Installation of a Driven Well

920.ILLUSTRATION J Sealing an Abandoned Well − Extending into a Creviced Formation

920.ILLUSTRATION K Sealing an Abandoned Dug or Bored Well

920.ILLUSTRATION L Sealing an Abandoned Well Extending into More Than One Water Bearing Formation

920.ILLUSTRATION M Sealing an Abandoned Buried Slab Bored Well

920.TABLE A Steel Casing and Liner Pipe Weights and Dimensions

920.TABLE B Plastic Casing and Liner Pipe Specifications

920.TABLE C Minimal Lateral Distances in Feet Between Water Wells, Closed Loop Wells, and Sources of Contamination