SUBPART F: SAFETY REQUIREMENTS